**MAINTENANCE AND INSPECTION OF PILOT LADDER**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Vessel Name:** |  |  | **Month/Year:** |  |
| **Voyage No:** |  |  |  |  |

## 

## General Inspection and Maintenance of Rope Pilot Ladder – Monthly & Before Use:

(The condition of the Rope Ladder shall be checked by the Chief Officer or the Nominated Person monthly and before use)

|  |  |  |  |
| --- | --- | --- | --- |
| **Pilot Ladder Identification (No.)** | **Date of Inspection / Maintenance** | **Result** | **Inspector (Name/Signature)** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**Inspection and Check Scopes:**

1. Check for signs of wear and tear or signs of damages.
2. Clear any present dirt and dust.
3. Ensure the steps and ropes are free of oil, grease and paint.
4. Ensure chokes and guard rings are present and in good condition.
5. Ensure vessel has enough spares to repair the ladder in case of deterioration or damage.
6. Tag and Identification Reference No. intact
7. Check flexible hoses are in good condition.