BATTERY LOG

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Vessel: |  |  | Date: |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **General Use Battery** | | | |  | **Radio Plant Battery** | | | |
| Cell No. | Cell Voltage | Date Renewed | Remarks |  | Cell No. | Cell Voltage | Date Renewed | Remarks |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| Charging Voltage | |  | Volt |  | Charging Voltage | |  | Volt |
| Room Temperature | |  | o C |  | Room Temperature | |  | o C |
| Note: Battery Renewal Interval is 5 years and to be done during dry-docking | | | |  | Note: Battery Renewal Interval is 5 years and to be done during dry-docking. | | | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Equipment | Battery Voltage | | Charging Voltage | Room Temp  o C | Date Renewed | Remarks |
| No.1 | No.2 |  |  |  |  |
| **Lifeboat Port Side** |  |  |  |  |  |  |
| **Lifeboat Stbd Side** |  |  |  |  |  |  |
| **Emerg Generator** |  |  |  |  |  |  |
| Note: 1. Battery Renewal Interval is 2 years.  2. Charging voltage to be measured from charger terminal during charging | | | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| Chief Engineer: |  | Electrician: |  |
| Signature: |  | Signature: |  |