**COW PRE-ARRIVAL CHECK LIST**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Vessel: |  |  | Voyage No: |  |
| Port: |  |  | Date/Time: |  |

|  |  |  |
| --- | --- | --- |
| Pre-arrival Procedure | | Tick |
| 1. | Cargo suitable for COW. |  |
| 2. | Terminal notified of COW plan \*\* and O2 content in cargo tanks. |  |
| 3. | COW line system isolated from Pre-Heater. |  |
| 4. | All hydrant valves for portable machines on COW line blanked. |  |
| 5. | All master valves to individual tanks and individual inlet valves to COW machines closed and lashed. |  |
| 6. | COW lines pressurized to COW working pressure MAWP. |  |
| 7. | All COW machines inspected and greased. |  |
| 8. | Pressure gauges on top discharge line, manifold, and COW main line checked and tested. |  |
| 9. | Prima Vac, Self-Stripping systems or equivalent, monitoring equipment checked. |  |
| 10. | Watch schedule adjusted for COW operation. |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Chief Officer:** |  |  | **Master:** |  |
| **Signature:** |  |  | **Signature:** |  |