**ECHO SOUNDER DEPTH COMPARISON FORM**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Vessel:** |  |  |  |  |

| **Date / Time** | **Position**  **(Lat & Long)** | **V/L’s Draft** | **UKC**  **(Echo Sounder)** | **Squat** | **Tide** | **Echo Sounder Depth** | **Charted Depth** | **Diff** | **Remarks** | **Rank & Signature** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |

**Note:**

1. Tide to be subtracted from UKC (unless it is a –ve tide). ESD = Draft + Squat + UKC – Tide
2. Performance of the echo sounder should be tested on all ranges and scales to verify recordings against depths shown on the chart **every voyage**.